Tilt Spring - Disassemble - Off Vehicle. Chevrolet PJJ 2000

For 1990-2009 cars

#### Tools Required

J 41352 Modular Column Holding Fixture

1. Check the steering column for accident damage. Refer to Steering Column Accident Damage Inspection - Off Vehicle .
2. Install the steering column and J 41352 into a vise.
3. Tilt the column in the UP position
4. Apply pressure onto the spring retainer (3).
5. Turn the spring retainer (3) clockwise and release to remove the spring retainer (3).
6. Remove the tilt spring (2) and the spring guide (1).
7. Remove the spring guide (1) from the tilt spring (2).