Rear Seat Back Cushion Replacement. Chevrolet PJJ 2001

For 1990-2009 cars

### Removal Procedure

1. Unlatch the rear seat back.
2. Tilt the rear seat back forward 50 degrees.
3. Unhook the rear seat outer retractor side belts from the rear seat back.
4. Remove the spacer (4) at the right side key pin (1).
5. Slide the rear seat back to the right .
6. Disengage the left key pin (5) from the left key slot (6).
7. Slide the rear seat back to the left.
8. Disengage the right key slot (3) from the right key pin (1).
9. Remove the rear seat back.

### Installation Procedure

1. Install the rear seat back.
2. Inspect the insulator (2) for proper installation.
3. Replace the insulator (2) if the insulator is damaged or missing.
4. Slide the rear seat back to the left.
5. Engage the right key slot (3) to the right key pin (1).
6. Slide the rear seat back to the right.
7. Engage the left key pin (5) to the left key slot (6).
8. Install the spacer (4) at the right side key pin (1).
9. Hook the rear seat outer retractor side belts to the rear seat back.
10. Latch the rear seat back.