Windshield Wiper Motor Cover Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

1. Remove the wiper arms. Refer to Wiper Arm Replacement.
2. Remove the plenum chamber water deflector. Refer to Plenum Chamber Water Deflector Replacement in Body Front End.
3. Disconnect the electrical connector from the wiper motor.
4. Remove the three screws and the wiper motor cover from the wiper motor.

### Installation Procedure

1. Install the wiper motor cover onto the wiper motor with the three screws.

Tighten
Tighten the three screws to 2 N·m (18 lb in).

2. Connect the electrical connector to the wiper motor.
3. Install the plenum chamber water deflector. Refer to Plenum Chamber Water Deflector Replacement in Body Front End.
4. Install the wiper arms. Refer to Wiper Arm Replacement.
5. Operate the wipers and inspect for proper operation.