Fastener Tightening Specifications. Chevrolet PJJ 2000

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Battery Cable to Battery Bolt | 16 N·m | 12 lb ft
Battery Retainer Bolt | 18 N·m | 13 lb ft
Commutator End Frame/Field Frame Assembly Through Bolts | 9 N·m | 80 lb in
Generator Mounting Bolt (2.4L) | 50 N·m | 37 lb ft
IDI Assembly To Cam Shaft Housing Cover Bolts (2.4L) | 22 N·m | 15 lb ft
Negative Battery Cable Terminal Nut | 2. N·m | 12 lb ft
Negative Battery to Transaxle Stud Nut | 25 N·m | 18 lb ft
Negative Battery Cable to Tray Bolt | 35 N·m | 26 lb ft
Positive Battery Cable Terminal Nut | 20 N·m | 15 lb ft
Positive Battery Cable to Starter Solenoid Nut | 12 N·m | 106 lb in
Spark Plugs (2.4L) | 18 N·m | 13 lb ft
Starter Lead Wire to Starter Solenoid S Terminal Nut | 2.5 N·m | 22 lb in
Starter Motor Mounting Bolt (2.4L) | 43 N·m | 32 lb ft
Starter Motor to Engine Bolt (2.4L) | 90 N·m | 66 lb ft
Starter Motor Solenoid to the S Terminal Nut | 3 N·m | 27 lb in