Recommended Materials (Waterleak Repair). Chevrolet PJJ 2000

For 1990-2009 cars

Application | Type of Material | GM Part Number
--- | --- | ---

• | Windshield

• | Rear Window

• | Quarter Window

Urethane Adhesive Caulking Kit

GM P/N 12346284 or the equivalent

- Metal Joints

Brushable, Paintable Seam Sealer

--

• | Ventilation Ducts

• | Drip Moldings

3M Auto Bedding and Glazing Compound or the equivalent

--

- Small Cracks and Pin Holes

3M Drip-Check Sealer or the equivalent

--

- Large Holes

3M All Around Autobody Sealant P/N 8500 or the equivalent

--

- Weatherstrips

Weatherstrip Adhesive

--

• | Bolts

• | Studs

• | Screws

Strip Caulk

--