Steering Wheel Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 1859-A Steering Wheel Puller

1. Disconnect the negative battery cable.

Caution: This vehicle is equipped with a Supplemental Inflatable Restraint (SIR) System. Failure to follow the correct procedure could cause the following conditions:

• | Air bag deployment

• | Personal injury

• | Unnecessary SIR system repairs

In order to avoid the above conditions, observe the following guidelines:

• | Refer to SIR Component Views in order to determine if you are performing service on or near the SIR components or the SIR wiring.

• | If you are performing service on or near the SIR components or the SIR wiring, disable the SIR system. Refer to Disabling the SIR System.

2. Disable the supplemental inflatable restraint (SIR) system. Refer to Disabling the SIR System in SIR.
3. Remove the steering wheel inflatable restraint module. Refer to Infl Rst Steering Wheel Module Replacement in SIR.
4. Remove the steering wheel nut (1).

Notice: When removing the steering wheel, use only the specified steering wheel puller. Do not hammer on the end of the steering column shaft. Hammering could loosen the plastic injections which maintain the steering column rigidity.

5. Remove the steering wheel using the J 1859-A Steering Wheel Puller.
6. Remove the steering wheel (2) from the steering column (3).

### Installation Procedure

1. Install the steering wheel (2) to the column (3).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the steering wheel nut (1).

Tighten
Tighten the steering wheel nut to 37 N·m (27 lb ft).

3. Install the steering wheel inflatable restraint module. Refer to Infl Rst Steering Wheel Module Replacement in SIR.
4. Enable the SIR system. Refer to Enabling the SIR System in SIR.
5. Connect the negative battery cable.