Scan Tool Data List. Chevrolet PJJ 2000

For 1990-2009 cars

#### Data List

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Ignition ON, Engine OFF, Transmission in Neutral or Park, and Brake Unapplied
ABS Active | ABS | No/Yes | No
ABS Relay Command | ABS | On/Off | On
ABS Relay Feedback | ABS | On/Off | On
ABS Warning Lamp | ABS | On/Off | Off
Brake Fluid Level | ABS | OK/Low | OK
Brake Switch Status | ABS | Applied/Released | Released
EBCM To PCM Requested | ETS | % | 90%
ETS Status | ETS | Enable/Disable | Enabled
ETS Active | ETS | Active/Inactive | Inactive
ETS Active Lamp | ETS | On/Off | Off
ETS Warning Lamp | ETS | On/Off | Off
ETS Disable Lamp | ETS | On/Off | Off
Ignition Voltage | ABS | Volts | 12V
Left Front Wheel Speed | ABS/ETS | mph/km/h | 0
Left Rear Wheel Speed | ABS/ETS | mph/km/h | 0
LF Inlet Valve Solenoid | ABS | Active/Inactive | Inactive
LF Outlet Valve Solenoid | ABS | Active/Inactive | Inactive
LR Inlet Valve Solenoid | ABS | Active/Inactive | Inactive
LR Outlet Valve Solenoid | ABS | Active/Inactive | Inactive
PCM To EBCM Delivered | ETS | % | 90%
Pump Motor Commanded State | ABS | On/Off | Off
Pump Motor Feedback State | ABS | On/Off | Off
Right Front Wheel Speed | ABS/ETS | mph/km/h | 0
Right Rear Wheel Speed | ABS/ETS | mph/km/h | 0
RF Inlet Valve Solenoid | ABS | Active/Inactive | Inactive
RF Outlet Valve Solenoid | ABS | Active/Inactive | Inactive
Rough Road Parameter | ABS | g | 0.00
RR Inlet Valve Solenoid | ABS | Active/Inactive | Inactive
RR Outlet Valve Solenoid | ABS | Active/Inactive | Inactive
Switched Battery Voltage | ABS | Volts | 12V
Vehicle Speed | ABS/ETS | mph/km/h | 0