Front Wheel Speed Sensor Wiring Harness Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle on a suitable hoist. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the connector from the front wheel speed sensor.
3. Remove the harness attaching clips (2) from the control arm (3) and the splash shield (1).
4. Lower the vehicle.
5. Remove the harness attaching clips from the strut tower.
6. Cut the wheel speed sensor wiring circuits within the main engine harness.
7. Strip the insulation on the engine harness leads and the new wheel speed sensor harness leads.

### Installation Procedure

1. Splice the sleeve provided in the jumper harness kit over each engine harness lead.
2. Install the new wheel speed sensor harness leads to the engine harness leads and crimp the connections. Make sure the wire colors match.
3. Heat shrink the tube lightly to seal the connection.
4. Install the harness attaching clip to the strut tower.
5. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
6. Install the harness attaching clips (2) to the control arm (3) and the splash shield (1).
7. Install the connector to the front wheel speed sensor.
8. Lower the vehicle.
9. Perform the ABS Diagnostic System Check.