Headlamp Bulb Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

1. Remove the upper air intake splash shield. Refer to Hood Close Out Filler Replacement in Body Front End.
2. Remove the lamp assembly.
3. Remove the socket. Complete the following steps:

3.1. | Turn the socket.

3.2. | Pull out the socket

Caution: Halogen bulbs contain gas under pressure. Handling a bulb improperly could cause it to shatter into flying glass fragments. To help avoid personal injury:

• | Turn off the lamp switch and allow the bulb to cool before changing the bulb.

• | Leave the lamp switch OFF until the bulb change is complete.

• | Always wear eye protection when changing a halogen bulb.

• | Handle the bulb only by its base. Avoid touching the glass.

• | Keep dirt and moisture off the bulb.

• | Properly dispose of the used bulb.

• | Keep halogen bulbs out of the reach of children.

4. Use the following procedure in order to disconnect the electrical connector:

4.1. | With one hand, grip the wiring harness end of the bulb that the electrical wires enter.

Do not grip the wires.

| Important: Do not grip the bulb glass.

4.2. | With the other hand, grip the base of the bulb.

4.3. | Carefully pull the bulb base apart from the wiring harness.

### Installation Procedure

1. Connect the bulb socket to the lamp harness connector.
2. Align the bulb flange notch with the lamp housing key way.
3. Insert the bulb into the lamp housing.
4. Turn the bulb into the housing until it is retained.
5. Install the lamp assembly. Refer to Headlamp Replacement.