Park and Tail Lamps Always On. Chevrolet PJJ 2000

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---

1

1. Turn the headlamp switch to the OFF position.
2. Disconnect the turn/hazard headlamp switch assembly connector C1.

Did all of the exterior lamps go out?

--

Go to Step 3

Go to Step 2

2 | Repair the short to battery positive voltage in CKT 9. Is the repair complete? | -- | Go to Exterior Lights System Check | --
3 | Replace the turn/hazard headlamp switch. Is the repair complete? | -- | Go to Exterior Lights System Check | --