Chime Inoperative. Chevrolet PJJ 2001

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
DEFINITION: All chime functions are inoperative.
1 | Did you review the Audible Warnings Operation and perform the necessary inspections? | -- | Go to Step 2 | Go to Symptoms - Audible Warnings

2

1. Turn OFF the ignition, with the key in the ignition.
2. Open the driver's door.

Does the chime sound?

--

Go to Testing for Intermittent and Poor Connections in Wiring Systems

Go to Step 3

3 | Do the courtesy lamps illuminate when the driver's door is opened? | -- | Go to Step 4 | Go to Courtesy or Dome Lamps Inoperative in Lighting Systems

4

1. Turn ON the ignition, with the engine OFF.
2. Turn ON the radio.
3. Adjust the radio balance and fade to the left front speaker.

Does the speaker operate properly?

--

Go to Step 5

Go to Speakers Inoperative - One or More in Entertainment

5 | Important: Perform the set up procedure for the radio. Refer to Radio Setup in Entertainment. Replace the radio. Refer to Radio Replacement in Entertainment. Did you complete the replacement? | -- | Go to Step 6 | --
6 | Operate the system in order to verify the repair. Did you correct the condition? | -- | System OK | Go to Step 3