Rear Brake Hose Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

Caution: Do not move the vehicle until a firm brake pedal is obtained. Air in the brake system can cause loss of brakes with possible personal injury.

Notice: Brake hoses should not be crimped at any point to prevent loss of brake fluid from any component.

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the tire and wheel. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
3. Disconnect the rear brake pipes (2,7) from the rear brake hose (5).

Do not bend the rear brake pipes (2,7).

4. Plug the rear brake pipes (2,7) to prevent fluid loss or contamination.
5. Remove the rear brake hose retainers (3,6) from the rear brake hose (5).
6. Remove the rear brake hose (5) from the vehicle.

### Installation Procedure

1. Install the rear brake hose (5) to the vehicle.
2. Install the rear brake hose retainers (3,6) onto the rear brake hose (5).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Connect the rear brake pipes (2,7) to the rear brake hose (5).

Tighten
Tighten the rear brake pipe fittings to 23 N·m (17 lb ft).

4. Install the tire and wheel. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
5. Lower the vehicle.
6. Bleed the hydraulic brake system. Refer to Hydraulic Brake System Bleeding.