Fog Lamps Inoperative - One. Chevrolet PJJ 2000

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the Lighting System Diagnostic System Check performed? | -- | Go to Step 2 | Go to the Lighting System Diagnostic System Check
2 | With the fog lamps turned on, test for positive battery voltage at terminal B of the fog lamp that is not working. Is battery voltage present? | -- | Go to Step 3 | Go to Step 4
3 | Test terminal A of the fog lamp for continuity to ground. Is ground present | -- | Go to Step 5 | Go to Step 6
4 | Repair the open in CKT 34 Is the repair complete? | -- | System OK | --
5 | Replace the fog lamp bulb. Is the repair complete | -- | System OK | --
6 | Repair the open in CKT 150. Is the repair complete? | -- | System OK | --