Front Seat Head Restraint Cover Replacement. Chevrolet PJJ 2001

For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 42214 Headrest Removal Kit

1. Raise the headrest (1) off of the seat back (4).
2. Move the seat back cover to the right side of the seat near the headrest in order to locate the headrest guide tube thru the holes in the top of the trim cover.

Perform the above action from behind the seat back (4).

3. Apply upward tension to the headrest (1).
4. Slide the tip of the J 42214 .
5. Push the J 42214 .
6. Apply upward tension to the headrest (1) in order to prevent the first clip from re-engaging.
7. Perform the previous 4 steps on the other headrest guide tube in order to remove the headrest assembly (1) from the seatback.

### Installation Procedure

1. Perform the following procedure in order to install the headrest (1).

1.1. | Insert the posts into the guide tubes.

1.2. | Push the headrest (1) to the lowest position.

2. Pull up on the headrest (1) in order to verify that the lock springs are engaged.

Performing the above action prevents the headrest (1) from being removed.