Door Lamp Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

1. From the rear of the dome lamp lens, insert a flat bladed tool (1) between the dome lamp lens and the headining trim finish panel (2).
2. Use the flat bladed tool in order to push the tab at the rear of the dome lamp lens forward. Disengage the tab from the headlining trim finish panel.
3. Pull the dome lamp lens rearward in order to disengage the 2 tabs at the front of the dome lamp lens.
4. Pull the bulb rearward to remove it from the socket.

### Installation Procedure

1. Push the bulb forward to install it to the socket.
2. Insert the 2 forward tabs on the dome lamp lens into the appropriate holes in the headlining trim finish panel (2).
3. Push at the rear of the dome lamp lens until the rear tab is fully seated in the headlining trim finish panel.