Scan Tool Data Definitions. Chevrolet PJJ 2000

For 1990-2009 cars

Use the Scan Tool Data Display Values and Definitions Information in order to assist in diagnosing vehicle malfunctions. Compare the vehicles actual scan tool data with the typical data display value table information. Use the data information in order to aid in understanding the nature of the problem when the vehicle does not match with the typical data display values.

The scan tool data values were taken from a known good vehicle under the following conditions:

• | The ignition switch is in the ON position.

• | The engine is not running.

• | The vehicle is in PARK.

### Battery Voltage

This voltage value refers to the battery system voltage.

### Ignition 1

The BCM uses this data in order to determine the position of the ignition switch. ON is displayed when the ignition switch is in the ON or CRANK position.

### Accessory

The BCM uses this data in order to determine the position of the ignition switch. ON is displayed when the ignition switch is in the ON or ACCY position.

### Key In Ignition

This information refers to whether or not the ignition key is inserted into the ignition switch. The BCM uses this data to perform chime functions. ON is displayed when the key is inserted into the ignition switch.

### Traction Switch

The BCM uses this input to determine the position of the traction control switch. ON is displayed when the enhanced traction system is active.

### A/C Request

The BCM uses this input to determine the position of the air conditioning switch. YES is displayed when a/c is requested.

### Rear Defog Switch

The BCM uses this input to determine the position of the rear defogger switch. ON is displayed when the rear defogger is on.

### Park Brake Switch

The BCM uses this input to determine the position of the rear park brake switch. ON is displayed when the park brake is applied.

### Brake Fluid Level Switch

The BCM uses this input to determine the position of the brake fluid level switch. ON is displayed when a low brake fluid condition exists.

### Low Coolant Level

The BCM uses this input to determine the position of the coolant level switch. ON is displayed when a low coolant level condition exists.

### Park (BTSI) Relay

This output displays whether or not the BCM is providing ground for the A/T shift lock control solenoid. ON is displayed when the BCM is providing ground for the solenoid.

### Park (BTSI) Relay Feedback

This input displays the state of the A/T shift lock control solenoid. ACTIVE is displayed when the BCM is commanding the solenoid to lock the gear select lever.

### Panic Horn Relay

This output displays whether or not the BCM is providing ground for the horn relay. ON is displayed when the BCM is providing ground for the relay.

### Panic Horn Relay Feedback

This input displays the state of the horn relay. When the horn switch is pressed, ACTIVE is displayed.

### Last 4 Dig. of GM Part #

This information refers to the last 4 digits of the GM BCM part number that is currently in the vehicle.

### Model Year

This information refers to the model year of the vehicle.

### Year Module Built

This information refers to the year that the BCM was built.

### Calibration ID

This information refers to how the BCM is calibrated. This information is for assembly plant use only.