Piston and Connecting Rod Disassemble. Chevrolet PJJ 2001

For 1990-2009 cars

#### Tools Required

J 43654 Piston Pin Retainer Remover/Installer

1. Mark orientation of the piston to the connecting rod.
2. Remove the piston rings using a piston ring expander.
3. Remove the connecting rod bearing inserts.
4. Use J 43654 to remove the piston pin retainers.
5. Remove the piston pin. The pin is a full-floating style and should slide from the piston.
6. Remove the piston from the connecting rod.