License Lamps Inoperative. Chevrolet PJJ 2000

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---

1

1. Turn the ignition switch to the ON position.
2. Turn the turn/hazard - headlamp switch assembly to the HEAD position.
3. Disconnect the license lamp connector.
4. Connect the test lamp between terminal A of the license lamp harness connector and ground.

Does the test lamp light?

--

Go to Step 2

Go to Step 3

2 | Connect the test lamp between terminal A and terminal B of the license lamp harness connector. Does the test lamp light? | -- | Go to Step 4 | Go to Step 5
3 | Repair open in CKT 9 between Splice 9B and terminal A on license lamp connector. Refer to Wiring Repairs Is repair complete? (Pontiac coupe license lamps will always be on when ignition key is on.) | -- |  | --
4 | Replace the license bulb. Is the repair complete? | -- | System OK | --
5 | Repair the open in CKT 150. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | System OK | --