Engine Mount Strut Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
3. Remove the right front splash shield. Refer to Wheelhouse Splash Shield Replacement in Body Front End
4. Remove the engine mount strut bolts.
5. Remove the engine mount strut.

### Installation Procedure

1. Install the engine mount strut.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the engine mount strut bolts.

Tighten
Tighten the strut bolts to 100 N·m (74 lb ft) + 90 degrees.

3. Install the right front splash shield. Refer to Wheelhouse Splash Shield Replacement in Body Front End
4. Lower the vehicle.
5. Connect the negative battery cable.

Tighten
Tighten the bolt to 16 N·m (12 lb ft).