Door Window Regulator Replacement. Chevrolet PJJ 2001

For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 9886-01 Regulator Handle Clip Remover

1. Place the door window regulator handle in the upward position.
2. Insert the J 9886-01 or an equivalent between the door window regulator handle and the door trim panel.
3. Push the J 9886-01 downward.
4. Remove the door window regulator handle (4).
5. Remove the door window regulator handle bearing plate.

### Installation Procedure

1. Install the retaining clip to the door window regulator handle (4).
2. Install the door window regulator handle bearing plate.
3. Place the door window in the closed position.
4. Push the door window regulator handle (4) in order to secure the retaining clip.