Front Floor Panel Carpet Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

1. Remove the driver and passenger front seats. Refer to Seat Replacement in Seats.
2. Remove the console assembly. Refer to Console Replacement in Instrument Panel, Gauges and Console.
3. Remove the rear quarter trim panel. Refer to the following procedures:

• | Trim Panel Replacement - Rear Quarter (2 Door)

• | Trim Panel Replacement - Rear Quarter (4 Door)

4. Remove the floor carpet retainers. Refer to Carpet Retainer Replacement.
5. Remove the floor carpet.

### Installation Procedure

1. Install the floor carpet.
2. Install the floor carpet retainers. Refer to Carpet Retainer Replacement.
3. Install the rear quarter trim panel. Refer to the following procedures:

• | Trim Panel Replacement - Rear Quarter (2 Door)

• | Trim Panel Replacement - Rear Quarter (4 Door)

4. Install the console assembly. Refer to Console Replacement in Instrument Panel, Gauges and Console.
5. Install the front seats. Refer to Seat Replacement in Seats.