Inside Rearview Mirror Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

1. Loosen the set screw in the base of the mirror.
2. Remove the mirror from the mounting pad.

### Installation Procedure

1. Install the mirror to the mounting pad.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Tighten the set screw that retains the mirror base to the mounting pad.

Tighten
Tighten the mirror set screw to 2 N·m(18 lb in).

3. Install the rearview mirror reading lamp electrical wiring harness, if applicable.