Horn Replacement. Chevrolet PJJ 2001

For 1990-2009 cars

### Removal Procedure

1. Remove Right Wheel House Splash Shield. Refer to Splash Shield Replacement - Wheelhouse.
2. Remove the screw (3) from the front impact bar (1).
3. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.
2. Install the screw (3) to the front impact bar (1).
3. Install the Right Wheel House Splash Shield. Refer to Splash Shield Replacement - Wheelhouse.