Lower Oil Pan Installation. Chevrolet PJJ 2001

For 1990-2009 cars

1. Apply a 2-3 mm wide by 0.5-1.5 mm high bead of P/N 97720043 sealant to the lower oil pan mating surface.
2. Install the lower oil pan.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the lower oil pan bolts and nuts in sequence.

Tighten
Tighten the lower oil pan bolts and nuts to 10 N·m (89 lb in).

4. Connect the oil level sensor.