DTC B2625. Chevrolet PJJ 2001

For 1990-2009 cars

Refer to Interior Lights Dimming Schematics .

### Circuit Description

The body control module (BCM) receives a variable voltage from the instrument panel lamp dimmer switch. The BCM uses this signal in order to vary the illumination level of the instrument panel lamps. The instrument panel dimming lamps output from the BCM is a pulse width modulated voltage supply used to light the instrument panel lamps. If a malfunction occurs in the instrument panel dimming lamps output circuit, this DTC is set.

### Conditions for Running the DTC

The park lamp input is active (park or headlamps on).

### Conditions for Setting the DTC

Any of the following conditions will set this DTC:

• | The instrument panel dimming lamps output is open for 125 milliseconds.

• | The instrument panel dimming lamps output is shorted to ground for 125 milliseconds.

• | The instrument panel dimming lamps output is shorted to battery positive voltage for 125 milliseconds.

### Action Taken When the DTC Sets

• | If the instrument panel dimming lamps output is open, the instrument panel lamps will not illuminate.

• | If the instrument panel dimming lamps output is shorted to ground, the instrument panel lamps will not illuminate.

• | If the instrument panel dimming lamps output is shorted to battery positive voltage, the instrument panel lamps will illuminate at full intensity.

### Conditions for Clearing the DTC

• | A current DTC B2625 will clear when the malfunction is no longer present and the ignition switch is cycled.

• | All BCM history codes clear after 100 ignition cycles with no current codes active during the 100 ignition cycles.

• | A scan tool can be used to clear the DTC.

### Diagnostic Aids

If the DTC is a history DTC, the malfunction may be intermittent. Try performing the tests while wiggling the wires and connectors. This may often cause the malfunction to appear.

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you perform the Diagnostic System Check - Lighting Systems ? | Go to Step 2 | Go to Diagnostic System Check - Lighting Systems

2

1. Turn the ignition switch to the on position.
2. Turn the headlamp switch to the on position.
3. Attempt to adjust the lighting intensity of the instrument lamp with the dimmer switch.

Do the instrument panel lamps stay on at full intensity?

Go to Step 3

Go to Step 4

3 | Repair a short to voltage in the instrument panel dimming lamps output circuit. Refer to Wiring Repairs in Wiring Systems. Did you complete the repair? | Go to Step 12 | --
4 | Are all of the instrument panel lamps inoperative? | Go to Step 5 | Go to Step 7
5 | Test for a short to ground or open in the instrument panel dimming lamps output circuit between the BCM and each individual lamp connected to the output circuit. Refer to Circuit Testing and Wiring Repairs in Wiring Systems. Did you find and correct the condition? | Go to Step 12 | Go to Step 6
6 | Inspect for poor connections at the harness connector of the body control module. Refer to Testing for Intermittent Conditions and Poor Connections and Connector Repairs in Wiring Systems. Did you find and correct the condition? | Go to Step 12 | Go to Step 11

7

1. Disconnect the affected component on the instrument panel dimming lamps circuit.
2. Connect a test lamp between ground and the instrument panel dimming lamp output circuit at the affected component.
3. Turn the ignition switch to the on position.
4. Turn the headlamp switch to the on posiiton.

Does the testlamp illuminate?

Go to Step 8

Go to Step 9

8 | Test for an open in the instrument panel dimming lamp ground circuit at the affected component. Refer to Circuit Testing and in Wiring Systems Did you find and correct the condition? | Go to Step 12 | Go to Step 10
9 | Repair the open in the instrument panel dimming lamp output circuit at the affected component. Refer to Wiring Repairs in Wiring Systems Did you complete the repair? | Go to Step 12 | --
10 | Replace the inoperative component which causes this DTC to be set. Refer to the appropriate repair procedure. Did you complete the replacement? | Go to Step 12 | --
11 | Important: Perform the set up procedure for the body control module. Replace the body control module. Refer to Body Control Module Replacement . Did you complete the replacement? | Go to Step 12 | --

12

1. Use the scan tool in order to clear the DTCs.
2. Operate the vehicle within the Conditions for Running the DTC as specified in the supporting text.

Does the DTC reset?

Go to Step 2

System OK