Catalytic Converter Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

## Catalytic Converter Replacement 2.4L

### Removal Procedure

Notice: Do not over-flex or damage the flex joint when moving the flex joint from the normal mounting position.

1. Raise the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Support the three way catalytic converter.
3. Support the exhaust manifold pipe assembly.
4. Remove the three way catalytic converter from the intermediate pipe.
5. Remove the three way catalytic converter from the exhaust manifold pipe assembly.
6. Remove the three way catalytic converter and seals.
7. Clean the flange surfaces.

### Installation Procedure

1. Install the three way catalytic converter seals.
2. Install the three way catalytic converter to the intermediate pipe assembly.
3. Install the three way catalytic converter to the exhaust manifold pipe assembly.
4. Lower the vehicle.