Enabling the SIR System. Chevrolet PJJ 2000

For 1990-2009 cars

1. Connect the passenger yellow 2-way connector located near the base of the steering column.
2. Install the connector position assurance (CPA) to the passenger yellow 2-way connector.
3. Connect the driver yellow 2-way connector located at the base of the steering column.
4. Install the connector position assurance (CPA) to the driver yellow 2-way connector.
5. Install the IP insulator panel. Refer to Instrument Panel Insulator Replacement in Instrument Panel, Gauges and Console.
6. Install the SIR Fuse in the fuse block.
7. Staying well away from both air bags, turn ON the ignition.

7.1. | The AIR BAG warning lamp will flash seven times.

7.2. | The AIR BAG warning lamp will then turn OFF.

8. Perform Diagnostic System Check - SIR if the AIR BAG warning lamp does not operate as described.