Stop Lamp Switch Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

1. Remove the right side insulator panel. Refer to Insulator Panel Replacement in Instrument Panel, Gauges and Console.
2. Disconnect the electrical connector (3) from the stoplamp switch (4).
3. Remove the stoplamp switch (4) from the bracket (1) by grasping the stoplamp switch and turning it 90 degrees counter clockwise while pulling toward the rear of the vehicle.

### Installation Procedure

1. Install the stoplamp switch (4) in the bracket (1) until the stoplamp switch (4) is seated on the bracket (1).
2. Connect the electrical connector (3) to the stoplamp switch (4).
3. Adjust the stoplamp switch. Refer to Stoplamp Switch Adjustment.
4. Install the right side insulator panel. Refer to Insulator Panel Replacement in Instrument Panel, Gauges and Console.