Steering Knuckle. Chevrolet PJJ 2000

For 1990-2009 cars

1. Inspect the ball stud tightness in the steering knuckle boss.

1.1. | Shake the wheel and feel for movement of the stud end or the castellated nut at the knuckle boss.

1.2. | Inspect the castellated nut fastener tightening specifications is an alternative method of inspecting for wear. A loose nut can indicate a bent stud or an opened-up hole in the knuckle boss.

2. Replace worn or damaged the ball joints and knuckles.