Rear Compartment Lamp Inoperative. Chevrolet PJJ 2000

For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
1 | Was the Lighting Systems Diagnostic System Check Performed? | Go to Step 2 | Go to A Diagnostic System Check - Lighting Systems
2 | Inspect the rear compartment courtesy lamp bulb. Is the bulb filiment open? | Go to Step 6 | Go to Step 3
3 | Use a testlamp connected to a good ground in order to test for battery positive voltage at terminal A of the rear compartment courtesy lamp connector. Does the testlamp light? | Go to Step 4 | Go to Step 7
4 | Use a testlamp connected to battery positive in order to test for ground at terminal A of the rear compartment courtesy lamp switch connector. (Ensure that the rear compartment lid is open.) Does the testlamp light? | Go to Step 5 | Go to Step 8
5 | Repair the open in CKT 737 between the courtesy lamp and the courtesy lamp switch. Refer to Wiring Repairs in Wiring Systems. Did you complete the repair? | System OK | --
6 | Replace the rear compartment courtesy lamp. Did you complete the repair? | System OK | --
7 | Inspect for poor connections at the rear compartment courtesy lamp connector and terminal X of harness connector C200. Refer to Testing for Intermittent and Poor Connections and Connector Repairs in Wiring Systems. Was a condition found and corrected? | System OK | Go to Step 11
8 | Inspect for poor connections at the rear compartment courtesy lamp switch connector. Refer to Testing for Intermittent and Poor Connections and Connector Repairs in Wiring Systems. Was a condition found and corrected? | System OK | Go to Step 9
9 | Test for an open in the ground CKT 150. Refer to Wiring Repairs in Wiring Systems. Did you find and correct the condition? | System OK | Go to Step 10
10 | Replace the rear compartment courtesy lamp switch. Refer to Rear compartment Lamp Switch Replacement. Did you complete the repair? | System OK | --
11 | Repair the open in CKT 1732 between splice S222 and the rear compartment courtesy lamp connector. Refer to Wiring Repairs in Wiring Systems. Did you complete the repair? | System OK | --