Fastener Tightening Specifications. Chevrolet PJJ 2000

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Air Inlet Screen Screw | 2 N·m | 18 lb in
Fender Bolt | 7 N·m | 62 lb in
Fender Center Bracket Bolt to Body | 1.6 N·m | 14 lb in
Fender Center Bracket Bolt to Fender | 3 N·m | 27 lb in
Fender Lower Bracket Bolt to Fender | 8 N·m | 66 lb in
Fender Lower Bracket Bolt to Radiator Side Support | 3 N·m | 27 lb in
Hood Headlamp Seal Screw (Pontiac Only) | 1 N·m | 12 lb in
Hood Hinge Bolt | 21 N·m | 15 lb ft
Hood Hinge Pivot Bolt | 20 N·m | 15 lb ft
Hood Latch Bolt | 10 N·m | 89 lb in
Hood Latch Release Cable Handle Screw | 27 N·m | 20 lb ft
Hood Latch Striker Bolt | 21 N·m | 15 lb ft
Hood Latch Support Bolt | 9 N·m | 80 lb in
Lower Tie Bar Bolt | 25 N·m | 18 lb ft
Splash Shield Bolt | 2 N·m | 18 lb in