Counter Gear Shaft Disassemble. Chevrolet PJJ 2001

For 1990-2009 cars

#### Tools Required

J 44749 Split Plate Bearing/Gear Puller

Important:

• | Only remove the bearings if replacing the bearings. Do not use the bearings again after removal.

• | You must also replace the race for the bearing being replaced.

1. Inspect the bearings for damage or wear. Refer to Bearings and Spacers Cleaning and Inspection .
2. Using a hydraulic press and the J 44749 (1), remove the countershaft intermediate case bearing. Use the flat side of the J 44749 against the bearing.
3. Using a hydraulic press and the J 44749 (1), remove the bearing from the front of the countershaft.