Shudder or Vibration During Acceleration. Chevrolet PJJ 2000

For 1990-2009 cars

Checks | Action
--- | ---
There is an excessive constant velocity (CV) joint angle. | Repair the CV joint angle.
There is a sticking spider assembly (inner CV joint). | Lubricate or replace the inner CV joint. Refer to Wheel Drive Shaft Inner Joint and Boot Replacement (Free Motion Joint-2.4L).
There is a sticking joint assembly (outer CV joint). | Lubricate or replace the outer CV joint. Refer to Wheel Drive Shaft Outer Joint and Boot Replacement (Free Motion Joint 2.4L).