Fuse Block Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

1. Remove the battery ground negative cable.
2. Remove the Instrument panel carrier. Refer to IP carrier Replacement in this section.
3. Remove the electrical connectors.
4. Remove the fuse block (1) from the tie bar, by pressing the retainer and pushing inward.
5. Remove the wire terminals from the fuse block.

### Installation Procedure

1. Install the wires and terminals to the fuse block (1).
2. Install the fuse block to the tie bar.
3. Install the electrical connectors.
4. Install the instrument panel carrier. Refer to IP Carrier Replacement in this section.
5. Install the battery ground negative cable.