Tail Lamp Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

1. Disconnect the tail lamp wire harness sockets (3).
2. Remove the tail lamp nuts (2).
3. Remove the tail lamp.

### Installation Procedure

1. Install the tail lamp.
2. Align the tail lamp to the deck lid applique.
3. Install the tail lamp nuts (2).

Tighten
Tighten the tail lamps nuts to 5 (44 lb in).

4. Connect the tail lamp wire harness sockets (3).