Power Sunroof Description. Chevrolet PJJ 2000

For 1990-2009 cars

The power sunroof features the following components:

• | A power sliding glass panel

• | A manually operated sunshade

The power sunroof is electrically operated from a two position rocker type switch. The rocker type switch is located in the headliner near the top center of the windshield. Perform the following procedure in order to put the sunroof glass into the vent position:

1. Turn the ignition switch to the ON position.
2. Press the control switch into the rearward position.
3. Release the control switch.

Perform the following procedure in order to completely open the sunroof and slide the glass back above the roof panel:

1. Place the sunroof glass into the vent position.
2. Press the control switch into the rearward position.
3. Release the control switch.

In order to close the sunroof glass, hold the control switch in the forward position until the glass closes. An express module at the front of the modular assembly causes the glass panel to stop in the following positions:

• | closed

• | vent

• | fully open

An electrical harness is routed along the left portion of the windshield header and down the left windshield pillar.

### Sunroof Maintenance

Do not use an abrasive cleaner on the sunroof glass window. Using an abrasive cleaner may scratch and permanently damage the tinted coating on the inside of the window.