BRAKE BLEEDING TOOL MODIFIED PRESSURE BLEEDING BRAKE SYSTEM. Oldsmobile Custom Cruiser 1989

For 1990-2009 cars

# BRAKE BLEEDING TOOL MODIFIED PRESSURE BLEEDING BRAKE SYSTEM

#### SUBJECT: BRAKE BLEEDING TOOL MODIFICATION

#### MODELS/YEARS: 1991 CUSTOM CRUISER AND BRAVADA

This bulletin describes a modification which must be made to existing tool J 35856. This tool is used when pressure bleeding the brake system. J 35856 'Proportioning Valve Depressor' has been replaced and superseded by J 39177 'Combination Valve Pressure Bleeding Tool' for the Kelsey Hayes combination valve on the above mentioned cars and trucks.

#### IMPORTANT: Failure to modify or replace J 35856 may result in an ineffective bleed or damage to the combination valve.

Dealers may order J 39177 to replace J 35856 or modify all J 35856 tools in the following manner:

1. Remove the red plastic handle from the tool.

2. Clamp the tool carefully but securely in a bench vise with the three prongs accessible.

3. File down the raised 'dimple" from the center prong until the surface area is smooth.

The removal of the 'dimple" is all that is necessary to modify the tool. Attach the label provided to the modified J 35856 tool. Three labels will be shipped to each dealership Service Manager.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.