ROUGH EDGE 1/4 BODY SIDE MLDG. (TAPE APPLY PROCEDURE). Oldsmobile Custom Cruiser 1992

For 1990-2009 cars

# ROUGH EDGE 1/4 BODY SIDE MLDG. (TAPE APPLY PROCEDURE)

#### SUBJECT: ROUGH EDGE ON REAR QUARTER BODY SIDE MOULDING (APPLY TAPE TO SIDE MOULDING PROCEDURE)

#### VEHICLES AFFECTED: 1991 BUICK "B" WAGON, 1992 "B" SEDAN

Application: 1991 Buick Roadmaster Wagon before VIN MW405519 and 1992 Roadmaster Sedan before VIN NR409466.

#### Condition:

----------- Potential for scrapes on hands when in area of rear wheelhouse area (i.e. washing rear tires, changing tires, etc.).

#### Cause:

------ Rough edge on body side moulding protrudes past rear wheelhouse flange into rear inner wheelhouse.

#### Correction:

----------- Apply protective tape to body side moulding as follows:

1. Remove 3 screws holding moulding to rear wheelhouse flange.

2. Remove moulding from vehicle by pushing down on upper edge of moulding and rotating lower edge of moulding away from vehicle body.

3. Clean both sides of flange on body side moulding that covers wheelhouse flange with adhesive cleaner such as 3M #08984 or equivalent.

4. Wrap 3M tape #5430 or equivalent over edge of flange on body side moulding.

#### IMPORTANT: Protect quarter panel from paint damage during moulding installation by lightly applying small pieces of protective tape (ie. 3M #5430, electrical tape, cloth body tape, etc.) to back side of upper corners of moulding. Be sure enough tape is exposed to allow for easy removal of tape after moulding is installed.

5. Reinstall moulding on vehicle by placing moulding on upper retainers, pushing moulding downward, rotating lower edge of moulding toward vehicle and releasing moulding.

6. Reinstall 3 screws through moulding into wheelhouse flange.

7. Repeat for opposite side.

If vehicle is being repaired under warranty use:

Labour Operation Number: B8400 Right Side B8401 Left Side

Labour Time: 0.3 Hours Per Side

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.