QUARTER WINDOW GLASS LOOSE REPLACE SWING OUT GLASS. Oldsmobile Custom Cruiser 1991

For 1990-2009 cars

# QUARTER WINDOW GLASS LOOSE REPLACE SWING OUT GLASS

#### SUBJECT: SWING OUT QUARTER WINDOW GLASS LOOSE AT HINGES (REPLACE SWING OUT GLASS)

#### VEHICLES AFFECTED: 1991-92 "B" CAR (WAGONS ONLY) CHEVROLET CAPRICE WAGON OLDSMOBILE CUSTOM CRUISER WAGON BUICK ROADMASTER WAGON

THIS BULLETIN HAS BEEN REVISED TO CORRECT P/N USAGE.**

#### CONDITION:

---------- Some customers may comment about swing out quarter window glass that becomes loose at the hinge area.

#### CAUSE:

------ Hinge bond material releases.

#### CORRECTION:

----------- Replace the swing out glass only, using the following part numbers and the procedure found in the Service Manual, Section 10-7.

P/N 12506797 Right Side P/N 12506798 Left Side

#### IMPORTANT: 1. Do not attempt to reglue the hinge to the glass.

2. Do not replace the complete quarter glass module to make this repair.

For vehicles repaired under warranty use:

Labour Operation: C-0530 Right Side C-0531 Left Side Labour Time: 0.3 Hr. 0.3 Hr.

** North American Export Sales (NAES) dealers reference: Chevrolet Division bulletin 92-289-10 Oldsmobile Division bulletin 92-T-130 Buick Division bulletin 92-10-61

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.