MOAN OR SQUEAK NOISE FROM HOOD STEERING SHAFT AREA,REPOSITION. Oldsmobile Custom Cruiser 1992

For 1990-2009 cars

# MOAN OR SQUEAK NOISE FROM HOOD STEERING SHAFT AREA,REPOSITION

#### SUBJECT: MOAN OR SQUEAK NOISE FROM UNDERHOOD STEERING SHAFT AREA (REPOSITION TOP BRAKE PIPE)

#### VEHICLES AFFECTED: 1992 "B" CAR CHEVROLET CAPRICE BUICK ROADMASTER

Condition: A moan or squeak noise may be heard on some 1992 B-cars coming from the underhood steering shaft area transmitted through the steering column into the vehicle passenger compartment. This condition is most noticeable while making parking lot maneuvers.

Cause: The ABS (Anti-Lock Brake System) pipe adjacent to the plastic stone shield may contact and load the underside of the shield, causing the shield to rub on the rubber center bushing inside the shield.

Correction: 1. With the engine running, turn the steering wheel from lock to lock. Leave the steering wheel in the position where the noise is most audible and turn off the engine. Visually inspect the area where the pipes are in contact with the shield as shown in Figure 1.

2. Carefully reposition the top brake pipe away from the shield. Use care not to kink or nick the brake pipe. It does not take much effort to reposition the pipe.

3. Repeat lock to lock turns to verify repair fix.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.