DIESEL ENGINE SPECIFICATION SERVICE MANUAL CORRECTION. Pontiac 6000 1982

For 1990-2009 cars

# DIESEL ENGINE SPECIFICATION SERVICE MANUAL CORRECTION

THE 4.3L V-6 DIESEL ENGINE PISTON CLEARANCE TO BORE (SELECTIVE) SPECIFICATION ON PAGE 6A6-44 IS INCORRECT. THE CORRECT SPECIFICATION FOR THE PISTON CLEARANCE TO BORE IS .076-102MM (.003-.004). NOTE THIS CORRECTION IN YOUR MANUAL.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.