UPDATE-REAR WHEEL ALIGNMENT SPECIFICATION. Pontiac 6000 1990

For 1990-2009 cars

# UPDATE-REAR WHEEL ALIGNMENT SPECIFICATION

#### VEHICLES AFFECTED: 1990 PONTIAC 6000 AWD (PAGE 6 REVISED)

Use the following rear wheel alignment specifications when checking or setting rear wheel alignment. Disregard any rear wheel alignment specifications for AWD in the 1990 Chevrolet/Pontiac Service Manual.

Rear Sum Toe 0.2 DEG /- 0.2 DEG (LH plus RH)

Rear Thrust Angle 0 DEG +/- 0.15 DEG

Rear Camber 0.4 DEG +/- 0.4 DEG

Rear Cross Camber 0 DEG +/- 0.6 DEG (LH plus RH)

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.