SERVICE MANUAL UPDATE SEC. 6 ROTATING ENG. IS NOT NECESSARY. Pontiac 6000 1990

For 1990-2009 cars

# SERVICE MANUAL UPDATE SEC. 6 ROTATING ENG. IS NOT NECESSARY

#### Subject: SERVICE MANUAL UPDATE - SECTION 6 ROTATING ENGINE - 3.1L (VIN T) ENGINE (CORRECTION TO PROCEDURES)

#### Models Affected: 1990 6000 MODELS

Any procedure or reference to "Rotating Engine" (3.1L engine) found in the 1990 6000 Service Manual is to be disregarded. There is no need or means of "Rotating Engine" to service any components on the 1990 Pontiac 6000.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.