RADIO STATIC/POOR RECEPTION REROUTE ANTENNA CABLE. Pontiac 6000 1985

For 1990-2009 cars

# RADIO STATIC/POOR RECEPTION REROUTE ANTENNA CABLE

1985 6000 STE

There have been some instances of misrouted radio antenna cables and/or the radio digital clock wire connector clipped incorrectly. These items may result in radio static or poor AM reception and an inoperative radio clock.

To repair this condition, remove the radio and reroute the radio antenna cable below the I.P. side window defogger tube and glove box. This will allow sufficient antenna cable length to permit its attachment to the radio.

The memory/dimming circuit (part of main harness) 2-pin female connector (black) may be trapped by the right hand main wire harness clip that fastens the main wire harness to the instrument panel (see attached sketch). The radio 2-pin male connector (white) will appear to be too short to connect to the female connector in the main harness. Take the female connector and wires out from under the I/P clip to permit a connection.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.