TOWING CHANGE INFORMATION. Pontiac 6000 1988

For 1990-2009 cars

# TOWING CHANGE INFORMATION

DISABLED VEHICLE TOWING CHANGE

#### MODELS AFFECTED 1988 PONTIAC 6000 SE --------------- (INCLUDING STATION WAGONS)

The 1988 6000 SE (including station wagons) must not be towed with sling-type equipped trucks from the front. Page 9 of the General Motors 1988 Passenger Car and Light Truck Towing Instructions Manual (T59) does not address this towing information.

The 1988 Pontiac 6000 SE (including station wagons) can be transported with either wheel-lift or rollback equipment.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.