CAMPAIGN: COLD START VALVE- THERMAL AND TIME SWITCH WIRING. Pontiac 6000 1986

For 1990-2009 cars

# CAMPAIGN: COLD START VALVE- THERMAL AND TIME SWITCH WIRING

GENERAL MOTORS HAS DETERMINED THAT SOME 1986 CHEVROLET CELEBRITY MODELS EQUIPPED WITH 2.8L MFI (RPO LB6) ENGINE MAY HAVE TWO CIRCUIT WIRES INTERCHANGED IN THE COLD START VALVE THERMAL AND TIME SWITCH. THIS CAN RESULT IN A GROUNDING OF THE COLD START INJECTOR POWER CIRCUIT. THIS GROUNDING CAN BLOW THE 10 AMP FUSE IN THE CRANK CAVITY. THEREAFTER, THE COLD START INJECTOR WILL NOT OPERATE CAUSING DIFFICULT OR NO STARTING. TO CORRECT THIS CONDITION, THE CIRCUIT WIRES WILL BE INSPECTED, AND IF REQUIRED, BE REVERSED AND THE "CRANK" FUSE REPLACED PER INSTRUCTIONS IN THIS BULLETIN. VEHICLES INVOLVED CERTAIN 1986 "A" CARS EQUIPPED WITH 2.8L MFI (RPO LB6) ENGINE BUILT WITHIN THE FOLLOWING BREAKPOINTS: PLANT MODEL FROM THROUGH OSHAWA (NO.2) CHEVROLET CELEBRITY G1100047 G1113682 INVOLVED VEHICLES HAVE BEEN IDENTIFIED BY VEHICLE IDENTIFICATION NUMBER COMPUTER LISTINGS. COMPUTER LISTINGS CONTAIN THE COMPLETE VEHICLE IDENTIFICATION NUMBER, OWNER NAME AND ADDRESS DATA, AND ARE FURNISHED TO THE INVOLVED DEALERS WITH THE CAMPAIGN BULLETIN. OWNER NAME AND ADDRESS DATA FURNISHED WILL ENABLE DEALERS TO FOLLOW-UP WITH OWNERS INVOLVED IN THIS CAMPAIGN. THESE LISTINGS MAY CONTAIN OWNER NAMES AND ADDRESSES OBTAINED FROM STATE MOTOR VEHICLE REGISTRATION RECORDS. THE USE OF SUCH MOTOR VEHICLE REGISTRATION DATA FOR ANY OTHER PURPOSE IS A VIOLATION OF LAW IN SEVERAL STATES. ACCORDINGLY, YOU ARE URGED TO LIMIT THE USE OF THIS LISTING TO THE FOLLOW-UP NECESSARY TO COMPLETE THIS CAMPAIGN. ANY DEALER NOT RECEIVING A COMPUTER LISTING WITH THE CAMPAIGN BULLETIN HAS NOT INVOLVED VEHICLES CURRENTLY ASSIGNED. OWNER NOTIFICATION OWNERS WILL BE NOTIFIED OF THIS CAMPAIGN ON THEIR VEHICLES BY CHEVROLET MOTOR DIVISION (SEE COPY OF OWNER LETTER INCLUDED WITH THIS BULLETIN). DEALER CAMPAIGN RESPONSIBILITY DEALERS ARE TO SERVICE ALL VEHICLES SUBJECT TO THIS CAMAPIGN AT NO CHARGE TO OWNERS, REGARDLESS OF MILEAGE, AGE OF VEHICLE, OR OWNER- SHIP, FROM THIS TIME FORWARD. WHENEVER A VEHICLE SUBJECT TO THIS CAMPAIGN IS TAKEN INTO YOUR NEW OR USED VEHICLE INVENTORY, OR IT IS IN YOUR DEALERSHIP FOR SERVICE IN THE FUTURE, YOU SHOULD TAKE THE STEPS NECESSARY TO BE SURE THE CAMPAIGN CORRECTION HAS BEEN MADE BEFORE RESELLING OR RELEASING THE VEHICLE. OWNERS OF VEHICLES RECENTLY SOLD FROM YOUR NEW VEHICLE INVENTORY ARE TO BE CONTACTED BY THE DEALER, AND ARRANGEMENTS MADE TO MAKE THE REQUIRED MODIFICATION ACCORDING TO INSTRUCTIONS CONTAINED IN THIS BULLETIN. PARTS INFORMATION PARTS REQUIRED TO COMPLETE THIS MODIFICATION ARE TO BE OBTAINED FROM GENERAL MOTORS WAREHOUSING AND DISTRIBUTION DIVISION (GMWDD). TO ENSURE THAT THESE PARTS WILL BE OBTAINED AS SOON AS POSSIBLE THEY SHOULD BE ORDERED FROM GMWDD ON A C.I.O. ORDER WITH NO SPECIAL INSTRUCTION CODE BUT ON AN ADVISE CODE (2). PART NUMBER DESCRIPTION QUANTITY 12004007 10 AMP MINI FUSE 1 SERVICE PROCEDURE 1. OPEN HOOD. 2. DISCONNECT NEGATIVE BATTERY CABLE. 3. REMOVE CONNECTOR FROM COLD START VALVE THERMAL AND TIME SWITCH (SEE FIGURE 1). 4. PULL RUBBER BOOT BACK FROM TERMINAL, INSPECT FOR PROPER WIRE ROUTING (SEE FIGURE 2), IF CORRECT GO TO STEP 8. 5. REMOVE TERMINALS FROM CONNECTOR BODY. 6. REINSTALL TERMINALS, MAKING SURE THE POSITION IS THE SAME AS SHOWN IN FIGURE 2. 7. REPLACE THE "CRANK" FUSE. (SEE FIGURE 3). 8. RECONNECT NEGATIVE BATTERY CABLE. 9. START ENGINE; THEN CHECK "CRANK" FUSE TO ASSURE CORRECT WIRING. 10. INSTALL CAMPAIGN COMPLETION LABEL AND CLOSE HOOD. CAMPAIGN IDENTIFICATION LABEL EACH VEHICLE MODIFIED IN ACCORDANCE WITH THE INSTRUCTIONS OUTLINED IN THIS PRODUCT CAMPAIGN BULLETIN WILL REQUIRE A "CAMPAIGN IDENTIFICATION LABEL." EACH LABEL PROVIDES A SPACE TO INCLUDE THE FIVE DIGIT DEALER CODE OF THE DEALER PERFORMING THE CAMPAIGN SERVICE. THIS INFORMATION MAY BE INSERTED WITH A TYPEWRITER OR BALLPOINT PEN. EACH "CAMPAIGN IDENTIFICATION LABEL" IS TO BE LOCATED ON THE RADIATOR CORE SUPPORT IN AN AREA WHICH WILL BE VISIBLE WHEN THE VEHICLE IS BROUGHT IN FOR PERIODIC SERVICING BY THE OWNER. APPLY "CAMPAIGN IDENTIFICATION LABEL" ONLY ON A CLEAN DRY SURFACE. CLAIM INFORMATION SUBMIT A PRODUCT CAMPAIGN CLAIM WITH THE INFORMATION INDICATED BELOW: ** * FAILED PARTS LABOR LABOR OTHER REPAIR PERFORMED FC PART NO. ALLOW FC OP HRS HRS O INSPECT NO FURTHER ACTION REQUIRED 00 V3430 .2 .1 O INSPECT REVERSE CIRCUIT WIRES AND REPLACE FUSE 1 12004007 ** 00 V3431 .2 .1 *CAMPAIGN ADMINISTRATIVE ALLOWANCE. **THE PARTS ALLOWANCE SHOULD BE THE SUM TOTAL OF THE CURRENT GMWDD DEALER NET PRICE PLUS 30% OF ALL PARTS REQUIRED FOR THE REPAIR. DEALERS WILL AUTOMATICALLY RECEIVE THE CORRECT LABOR AND MATERIAL ALLOWANCE PRICE PLUS 30% OF ALL PARTS REQUIRED FOR THE REPAIR. DEALERS WILL AUTOMATICALLY RECEIVE THE CORRECT LABOR AND MATERIAL ALLOWANCE BASED ON THE LABOR OPERATION PERFORMED. REFER TO THE CHEVROLET CLAIMS PROCESSING MANUAL FOR DETAILS ON PRODUCT CAMPAIGN CLAIM SUBMISSION. CHEVROLET MOTOR DIVISION GENERAL MOTORS CORPORATION

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.