HARSH 3-2 DOWNSHIFT AT HOT OUTSIDE TEMP-NEW SRTA MODEL. Pontiac 6000 1990

For 1990-2009 cars

# HARSH 3-2 DOWNSHIFT AT HOT OUTSIDE TEMP-NEW SRTA MODEL

New SRTA model to correct a harsh 3-2 downshift in hot outside temperatures for the 3.1L (VIN V) turbo W-Car. The replacement of the existing transaxle with the SRTA model listed under "SERVICE PARTS INFORMATION" is the only way to correct the harsh 3-2 downshift concern.

#### IMPORTANT:

Reference Figure 1 for correct vacuum line connections.

SERVICE PARTS INFORMATION:

Transaxle Part Number Description Model Year Model Usage

8676915 Transaxle - SRTA 1990 OLAH, OYRH

Parts are currently available from CANSPO.

#### SERVICE NOTES:

Model OYRH is the replacement for the OLAH model.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.