REAR LID LUGGAGE RACK DEALER INSTALLATION GUIDELINES. Pontiac 6000 1986

For 1990-2009 cars

# REAR LID LUGGAGE RACK DEALER INSTALLATION GUIDELINES

ALL 1986 MODELS

Federal Motor Vehicle Safety Standard 108 contains rear visibility requirements for the high mounted center stop lamp. Care must be exercised to install only luggage racks that do not violate this Standard. Use only GM approved luggage racks mounted per instructions provided in the accessory package.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.