125-125C ROUGH NEUTRAL TO DRIVE, NEW CLUTCH WAVE PLATE. Pontiac 6000 1984

For 1990-2009 cars

# 125-125C ROUGH NEUTRAL TO DRIVE, NEW CLUTCH WAVE PLATE

SOME 1982 THRU 1984 THM 125/125-C TRANSAXLE MAY EXHIBIT A ROUGH NEUTRAL TO DRIVE ENGAGEMENT CONDITION. BEGINNING DECEMBER, 1983, A NEW FORWARD CLUTCH WAVE PLATE, PART NUMBER 8652126 WENT INTO PRODUCTION. ( REFER TO THE CHART BELOW FOR MODEL AND SERIAL NUMBER APPLICATION.) ALL 1982 AND 1983 MODELS AND ALL 1984 UNITS ASSEMBLED PRIOR TO THESE BREAK POINTS HAVE PAST MODEL WAVE PLATES. WHEN SERVICING ANY 1982 THRU 1984 MODEL THM 125/125C TRANSAXLE FOR THIS ROUGH NEUTRAL TO DRIVE CONDITION ORDER PART NUMBER 8652126. REFER TO THE SERVICE MANUAL FOR REMOVAL AND REPLACEMENT OF THE FORWARD CLUTCH WAVE PLATE. MODEL SERIAL NO. MODEL SERIAL NO MODEL SERIAL NO CA 2724 EL 4201 HY 29466 CB 221301 EM 3342 PD 2508 CC 1219 CE 77876 EN 4984 PE 64573 CF 7881 EP 2427 PF 31776 CT 4840 EQ 136060 PG 63043 EB 3276 HC 2086 PJ 8148 EF 7642 HM 2980 PW 82620 EI 6450 HP 1154 EJ 1006 HS 16495 EK 11147 HX 6250 MODEL JULIAN DATE

BF 082 BL 082 OP 082

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.