FRONT SEAT BACK NOISY AR9 OPTION FRONT SEATS. Pontiac 6000 1987

For 1990-2009 cars

# FRONT SEAT BACK NOISY AR9 OPTION FRONT SEATS

FRONT SEAT BACK NOISY

#### MODELS AFFECTED 1987 6000 MODELS WITH FRONT BUCKET --------------- RECLINING SEAT - OPTION AR9

Owners of some 1987 6000 models with front bucket reclining (European Style) seats, option code AR9, may comment on a seat back noise, pop, rattle, or creak at the seat back pivot arm area.

To eliminate the noisy condition replace the pivot bolt with a new one, P/N 20642321 and bushing, P/N 17960700.

#### WARRANTY INFORMATION:

Labor Operation: T1256

Labor Time : .2 Hours per seat

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.